<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="-1.524" y1="0" x2="33.071" y2="0" width="0" layer="20"/>
<wire x1="33.071" y1="0" x2="33.071" y2="33.391" width="0" layer="20"/>
<wire x1="33.071" y1="33.391" x2="-1.524" y2="33.391" width="0" layer="20"/>
<wire x1="-1.524" y1="33.391" x2="-1.524" y2="0" width="0" layer="20"/>
<text>VCC</text>
<text>GND</text>
<text>Vin</text>
<text>GND</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>TX</text>
<text>RX</text>
<text>VCC</text>
<text>1</text>
<text>2</text>
<text>24</text>
<text>23</text>
<text>11</text>
<text>12</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="B130-13-F">
<packages>
<package name="SMA">
<description>&lt;b&gt;SMA&lt;/b&gt; CASE 403D-02&lt;p&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MBRA340T3-D.PDF</description>
</package>
</packages>
</library>
<library name="LM3480IM3-3.3_NOPB">
<description>&lt;100 mA, SOT-23, Quasi Low-Dropout Linear Voltage Regulator&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P237X112-3N">
<description>&lt;b&gt;DBZ (R-PDSO-G3)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X12">
<description>&lt;h3&gt;Plated Through Hole - 2x12&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:24&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="KSR223GLFG">
<description>&lt;Subminiature Tact Switch for SMT&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="KSR">
<description>&lt;b&gt;KSR&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="BeagleBone_Blue_R3">
<description>Generated from &lt;b&gt;BeagleBone_Blue.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="TP12R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="RN4870-V_RM118">
<description>&lt;Microchip RN4870-V/RM118 Bluetooth Chip 4.2&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="RN4870">
<description>&lt;b&gt;RN4870&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="B130-13-F" package="SMA" value="B130-13-F">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Diode, Schottky, 1a, 30v, Do-214ac-2, Full Reel "/>
<attribute name="MF" value="Multicomp"/>
<attribute name="MP" value="B130-13-F"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="DO-214 Multicomp"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="IC1" library="LM3480IM3-3.3_NOPB" package="SOT95P237X112-3N" value="LM3480IM3-3.3_NOPB">
<attribute name="DESCRIPTION" value="100 mA, SOT-23, Quasi Low-Dropout Linear Voltage Regulator"/>
<attribute name="HEIGHT" value="1.12mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LM3480IM3-3.3/NOPB"/>
<attribute name="MOUSER_PART_NUMBER" value="926-LM3480IM33.3NOPB"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=926-LM3480IM33.3NOPB"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="5361530P"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/5361530P"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="2X12" value="CONN_12X2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="KSR223GLFG" package="KSR" value="KSR223GLFG">
<attribute name="DESCRIPTION" value="Subminiature Tact Switch for SMT"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="C &amp; K COMPONENTS"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KSR223GLFG"/>
<attribute name="MOUSER_PART_NUMBER" value="611-KSR223GLFG"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=611-KSR223GLFG"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="BeagleBone_Blue_R3" package="TP12R" value="TPTP12R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="BeagleBone_Blue_R3" package="TP12R" value="TPTP12R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="RN4870-V_RM118" package="RN4870" value="RN4870-V_RM118">
<attribute name="DESCRIPTION" value="Microchip RN4870-V/RM118 Bluetooth Chip 4.2"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RN4870-V/RM118"/>
<attribute name="MOUSER_PART_NUMBER" value="579-RN4870-V/RM118"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=579-RN4870-V%2FRM118"/>
<attribute name="NAME"/>
<attribute name="RS_PART_NUMBER" value="1238535"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1238535"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ADFS">
<contactref element="IC1" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="31"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="32"/>
<contactref element="J1" pad="4"/>
<contactref element="RESET" pad="2"/>
<contactref element="J3" pad="24"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="5"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="4"/>
<contactref element="J3" pad="19"/>
<contactref element="J3" pad="21"/>
<contactref element="J1" pad="1"/>
<contactref element="RX" pad="A"/>
<contactref element="S1" pad="A"/>
<contactref element="S2" pad="A"/>
<contactref element="TX" pad="A"/>
<contactref element="J4" pad="2"/>
<contactref element="J4" pad="4"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="VBAT">
<contactref element="D2" pad="C"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="17"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="P1_0">
<contactref element="U1" pad="16"/>
<contactref element="J3" pad="3"/>
<contactref element="S2" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="15"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="14"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="13"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="P1_1">
<contactref element="U1" pad="12"/>
<contactref element="J3" pad="11"/>
<contactref element="S1" pad="C"/>
</signal>
<signal name="P2_7">
<contactref element="U1" pad="11"/>
<contactref element="J3" pad="13"/>
<contactref element="TX" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="U1" pad="9"/>
<contactref element="J3" pad="15"/>
</signal>
<signal name="N$9">
<contactref element="TP1" pad="TP"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="TP2" pad="TP"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="22"/>
<contactref element="J1" pad="2"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="23"/>
<contactref element="J1" pad="3"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="30"/>
<contactref element="J3" pad="20"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="29"/>
<contactref element="J3" pad="18"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="28"/>
<contactref element="J3" pad="16"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="27"/>
<contactref element="J3" pad="14"/>
</signal>
<signal name="P3_3">
<contactref element="U1" pad="26"/>
<contactref element="RX" pad="C"/>
<contactref element="J3" pad="12"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="25"/>
<contactref element="J3" pad="10"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="24"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="21"/>
<contactref element="RESET" pad="1"/>
<contactref element="J3" pad="22"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="19"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="5"/>
<contactref element="J3" pad="17"/>
</signal>
<signal name="MODE">
<contactref element="U1" pad="18"/>
<contactref element="J3" pad="23"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
