{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":47,"n_cols":8,"rows_kept":47}
[]
[]
[]
[]
[null,null,"CN1",null,null,"X2"]
[null,null,16,"GND",null,6,null,"BLK"]
[null,null,17,"3.3V",null,9,null,"RED"]
[null,null,18,"PWR_RLY_ON","RE7",13,null,"RED"]
[null,null,19,"PWR_RLY_OFF","RG9",14,null,"RED"]
[null,null,20,"HARAKIRI_ON","RB0",15,null,"RED"]
[null,null,21]
[null,null,22,"12V PIC Power",null,"PWR",null,"RED"]
[null,null,23,"12V_PRESENCE","RB15",16,null,"RED"]
[null,null,24,"BATT_VOLTAGE_IN","RB1",7,null,"RED"]
[null,null,25,"GND",null,8,null,"BLK"]
[null,null,26,"GND",null,"PWR",null,"BLK"]
[]
[null,null,"CN2",null,null,"X3"]
[null,null,32,"GND","GND",4,null,"BLK"]
[null,null,33,"3.3V","3V3",1,null,"RED"]
[null,null,34,"Current sense SDA","RD2",9,null,"RED"]
[null,null,35,"Current sense SCL","RD3",10,null,"RED"]
[null,null,36,null,"N/C"]
[null,null,37,"12V","N/C"]
[null,null,38,"GND","N/C",null,null,"BLK"]
[null,null,39,"LORA Aux","RD4",11,null,"RED"]
[null,null,40,"LORA TX  (PIC RX)","RF4",2,null,"RED"]
[null,null,41,"LORA RX (PIC TX)","RF5",3,null,"RED"]
[null,null,42,"LORA M1","RD5",12,null,"RED"]
[null,null,43,"LORA M0","RD6",13,null,"RED"]
[]
[]
[null,null,"LORA"]
[null,null,37,"12V","orange"]
[null,null,38,"GND","orange-blanc"]
[null,null,39,"LORA Aux","vert"]
[null,null,40,"LORA TX  (PIC RX)","bleu","PIC 2"]
[null,null,41,"LORA RX (PIC TX)","bleu-blanc","PIC3"]
[null,null,42,"LORA M1","brun"]
[null,null,43,"LORA M0","brun-blanc"]
[{"$nulls":4},"vert-blanc"]
[]
[null,null,"Sensor"]
[null,null,26,"GND"]
[null,null,27,"3.3V"]
[null,null,28,"Current sense SDA"]
[null,null,29,"Current sense SCL"]